**UNIT – IV**

**RATE ANALYSIS-II:**

Roofing: a) R.C.C. roof 10cm thick, two courses of flat tiles to top.

b) A.C. corrugated sheet roofing on steel purlins.

Plastering : a) With L.M. (1:1.5) 2 coats (20mm thick)

b) C.M. (1:4) 12mm thick.

Pointing: a) With C.M. (1:3) flush pointing to R.R. Masonry.

b) C.M. (1:3) for brick masonry.

Painting: a) Whitewashing and colour washing of walls: 2 coats.

b) Painting iron and woodwork: 3 coats.

Woodwork: Panelled doors and windows.

Road work: W.B.M. road with bituminous carpet 20mm thick.









